I patched the following things for my mix of „In the meantime”:

Inserts outboard:
dbx 160A on Wurlitzer keys: 
-Threshold: +2dB
-Ratio: 3:1
-Output gain: +3dB

Empirical Labs Distressor on lead vocal:
-Ratio 4:1
-Input gain: 4
-Attack: 0
-Release: 6
-Output gain: 7
-British Mode on.
-Audio through Dist2 mode.

API 2500 on mix bus:
-Threshold +6dB
-Attack: 0.03
-Ratio: 6:1
-Release: 0.2
-Knee: hard
-Thrust: normal
-Type: old
-…

See attached screenshots.

Inserts plugins:
Waves De-Esser plugins on all vocals (except BG4 and BG4D) due to lack of actual outboard de-essers.

See attached screenshots.

Sonnox Oxford TransMod on guitar. No screenshot attached, forgot to make one and don’t own the plugin. Ratio was I believe 0.14 transient expansion.

Effect sends:

TC Electronic M3000 on all vocals: sent via aux 1-2 on Neve console. Preset „1 Bar Snare Tap” with only high dampening changed to -5dB from (I think) 12dB.

Echoboy on Electric Guitar 1a: sent via aux 3-4 on Neve console to Pro Tools. See attached screenshot.